
	x8dtl motherboard (PCIe bold) Ubuntu 18.04
slot#          6 5 4 3 2 1
4-in-1 adapter 0 0 1 0 0 0
Number RX-570  1 1 2
	Device Topology (AMD)	PCI-E, 01:00.0
Device Topology (AMD)	PCI-E, 03:00.0
Device Topology (AMD)	PCI-E, 06:00.0
Device Topology (AMD)	PCI-E, 08:00.0

	Number RX-570  1 0 3

	
	Device Topology (AMD) PCI-E, 03:00.0
Device Topology (AMD) PCI-E, 06:00.0
Device Topology (AMD) PCI-E, 07:00.0
Device Topology (AMD) PCI-E, 08:00.0

	Number RX-570  1 0 2


	Device Topology (AMD) PCI-E, 03:00.0
Device Topology (AMD) PCI-E, 06:00.0
Device Topology (AMD) PCI-E, 08:00.0
clinfo version 2.2.18.03.26



Windows version of clinfo from Oblomov at github: 2-2-18-4-6 x64
	TB85 motherboard    Ubuntu 18.04
Slot#          6 5 4 3 2 1
Nvidia GTX     1 1 1 1 1 1
X16              X


	Device Topology (NV) PCI-E, 01:00.0
Device Topology (NV) PCI-E, 02:00.0
Device Topology (NV) PCI-E, 03:00.0
Device Topology (NV) PCI-E, 04:00.0
Device Topology (NV) PCI-E, 05:00.0
Device Topology (NV) PCI-E, 06:00.0
clinfo version 2.2.18.03.26



	H110BTC motherboard  Ubuntu 18.04
Slot#      13 12 11 10  9  8  7  6  5  4  3  2  1
Nvidia GTX  1  1  1  1  0  0  0  1  1  1  0  1  1
X16                  x





	Device Topology (NV) PCI-E, 05:00.0
Device Topology (NV) PCI-E, 01:00.0
Device Topology (NV) PCI-E, 04:00.0
Device Topology (NV) PCI-E, 02:00.0
Device Topology (NV) PCI-E, 03:00.0
Device Topology (NV) PCI-E, 0a:00.0
Device Topology (NV) PCI-E, 0b:00.0
Device Topology (NV) PCI-E, 0e:00.0
Device Topology (NV) PCI-E, 08:00.0
clinfo version 2.2.18.03.26



	TB85 motherboard  Windows 10x64 s9x00
Slot#          6 5 4 3 2 1
ATI Firepro    1 1 1 1 1 1
X16              X

	Device Topology (AMD) PCI-E, 05:00.0
Device Topology (AMD) PCI-E, 06:00.0
Device Topology (AMD) PCI-E, 01:00.0
Device Topology (AMD) PCI-E, 04:00.0
Device Topology (AMD) PCI-E, 03:00.0
Device Topology (AMD) PCI-E, 02:00.0
clinfo version 2.2.18.04.06



	Area51 R4 Windows 10x64
Slot#    6  5 4 3 2 1
X16      x  x x x   x
[bookmark: _GoBack]Nvidia   1    1
	Device Topology (NV) PCI-E, 17:00.0
Device Topology (NV) PCI-E, 65:00.0
clinfo version 2.2.18.04.06



